E-Soar Plus 3.0.0 configured for transmitters without sliders e.g. Q X7
=======================================================================

This is a lightly modified version of ESP 3.0.0 to work with lower end tx's which lack sliders.

Changes from published ESP 3.0.0:

* Motor control is SC, down for idle, push forward for power. (CH18).
* Camber is fixed. (CH20)

Configuration and operation are exactly as described in E-Soar Plus 3.0.

- Mike Shellim 28 August 2021